# esp32-wifi-manager

## Connected to:

## Manual connect

ADD (HIDDEN) SSID

## or choose a network...

## Manual Connection

## Password for

## Connecting to

You may lose wifi access while the esp32 recalibrates its radio. Please wait until your device automatically reconnects. This can take up to 30s.

### Success!

### Connection failed

Please double-check wifi password if any and make sure the access point has good signal.

##

## IP Address

IP Address:
Subnet Mask:
Default Gateway:

Are you sure you would like to disconnect from this wifi?

# Audio output

I2S
SPDIF
Bluetooth

# Player name

# Optional setting (e.g. for LMS IP address)

# Squeezelite command to run

squeezelite -o I2S -b 500:2000 -d all=info -M esp32

# Start Squeezelite

Signal | GPIO pin
--- | ---
I2S |
I2S Bit clock |
I2S Word select |
I2S Data |
SPDIF |
SPDIF Bit clock |
SPDIF Word select |
SPDIF Data |

# Check for firmware upgrade

Firmware version | IDF version | Release date | HW platform | Branch | Flash this FW
--- | --- | --- | --- | --- | ---

## Firmware URL:

0%

squeezelite-esp32, © 2019, philippe44, sle118, daduke
Licender under ???

This app would not be possible without the following libraries:

- esp32-wifi-manager, © 2017-2019, Tony Pottier. Licensed under the MIT License.
- SpinKit, © 2015, Tobias Ahlin. Licensed under the MIT License.
- jQuery, The jQuery Foundation. Licensed under the MIT License.
- cJSON, © 2009-2017, Dave Gamble and cJSON contributors. Licensed under the MIT License.